**Leica Freeware Viewer**

See link below for downloading a free LAS X offline viewer.  You can open the .lif files and view z stacks by scrolling through them and show max intensity projections. You will not have 3D viewer capabilities.

[https://webshare.leica-microsystems.com/latest/core/widefield/](https://urldefense.com/v3/__https:/webshare.leica-microsystems.com/latest/core/widefield/__;!!HXCxUKc!1EculZBMVurp5g_52qpddPf0e1PkDlg2syNNmyhmEbnalqJk3m7YRvDZ1vn4eDuSRelPcDhEjv_ZG3hASWAUMeRTDtvFUF0b$)

Graphical user interface, application

Description automatically generated

1. Select and download the LASX\_Office\_1.4.4\_26810.zip
2. Extract the ZIP Files.
3. You must be logged into an administrative account and close all Windows applications.
4. Double click on the Setup.exe file and follow the prompts.