**Stellaris 5 Start-Up Procedure**

1. Turn Power Button (#1) to the ON (“I”) position.
2. Turn Laser Button (#2) to the ON (“I”) position.

**DO NOT TURN THE KEY.** Leave the key in the vertical position.

1. Turn the Computer (#3) ON. The computer will take several minutes to initialize.
2. Log into the software and double click on the **LASX** icon.

**Select OK** to initialize the Leica Application Suite X

Configuration: machine.xlhw

Microscope: DM18

1. Select the **Laser Overview** icon to turn the laser on.



Change the **Power State** for each laser from OFF to ON.

 Diode 405 (UV Light)

 Diode 448 (Visible)

 WLL (Supercon) 485-685

The WLL will take a few seconds to recognize and turn on.

 Leave the WLL at 85% Maximum Power.

**Stellaris 5 Shut-Down Procedure**

1. Exit the LASX software and shut down the computer.
2. Turn the Laser Button (#2) to the OFF (“O”) position.
3. Turn the Power Button (#1) to the OFF (“O”) position.